Attached is the connection and power supply requirements for the DIN input power on the PB-503.

OUTPUT: +10 VDC 2 A, +20 VDC 700 mA, -20 VDC 700 mA with assembly male 5 pin din plug (PIN 1: -20 VDC, PIN 2: COM+Ground, PIN 3: +20 VDC, PIN 4: no connection, PIN 5: +10 VDC)